**Schematic Errata**

Team 4: Dylan Burk, John Estes, Ryan Hopson, Taylor Neyland

MCLR# (pin 1 of SV1) and RTS# (pin 6 of FTDI) need to be connected.

RXD (pin 5 of FTDI and connected to MCUTX) and RF0 (pin 1 of H1) need to be connected.

The left sides of R6 and R7 need to be connected with a jumper wire. It is shown in the schematic but not printed on the circuit board.

DACCS# (connected to pin 3 of U4) should be connected to RD0 (pin 1 of H2).